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SECTION 900


NOTICE TO CONTRACTORS:
Sealed bids will be received by the Board of Supervisors of Jasper County in Bay Springs, Mississippi until 10:00 A.M., on Tuesday, September 8, 2026, and shortly thereafter publicly opened for the construction of 0.089 miles of BRIDGE & APPROACHES on the CR 35 being known as Local System Bridge Program (LSBP) Project No. LSBP-31(22) in Jasper County Mississippi.


PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS

	ROADWAY ITEMS:
	QUANTITY
	UNIT

	MOBILIZATION
	1.000
	LS

	CLEARING AND GRUBBING
	1.000
	LS

	REMOVAL OF BRIDGE @ STA. 12+85.43
	1.000
	UN

	BORROW EXCAVATION (F.M.E.) (CONTRACTOR FURNISHED) (CLASS 9)
	850.000
	CY

	EXCESS EXCAVATION (FM)
	323.000
	CY

	GRANULAR MATERIAL (LVM), (CLASS 9, GROUP B )
	684.000
	CY

	SIZE 1 STABILIZER AGGREGATE, COARSE
	79.000
	CY

	GUARD RAIL, "W" BEAM COMPLETE IN PLACE
	100.000
	LF

	GUARD RAIL, BRIDGE END SECTION, TYPE I THRIE BEAM
	4.000
	EA

	GUARD RAIL, TERMINAL END SECTION
	4.000
	EA

	ROADWAY CONSTRUCTION SURVEYING
	1.000
	LS

	RIGHT-OF-WAY MARKERS (TYPE II )
	10.000
	EA

	MAINTENANCE OF TRAFFIC
	1.000
	LS

	ADDITIONAL CONSTRUCTION SIGNS
	0.000
	SF

	REFLECTORIZED TRAFFIC WARNING SIGN WITH SUPP PLATE (ENCAPSULATED LENS)
	2.000
	EA

	REFLECTORIZED TRAFFIC OBJECT MARKER (ENCAPSULATED LENS) (TYPE 3 )
	4.000
	EA



	EROSION CONTROL ITEMS:
	
	

	REMOVE AND RELAY RIPRAP
	500.000
	SY

	AGRICULTURAL LIMESTONE
	1.340
	TON

	COMMERCIAL FERTILIZER ( 13:13:13)
	0.670
	TON

	SEEDING
	0.670
	AC

	VEGETATIVE MATERIALS FOR MULCH
	2.010
	TON

	SOLID SODDING
	130.000
	SY

	TEMPORARY SILT FENCE (TYPE II ) (AOS 0.15-0.84 )
	1,300.000
	LF

	WATTLES, 20"
	300.000
	LF

	LOOSE RIPRAP, 200 LB.
	100.000
	TON

	LOOSE RIPRAP, 300 LB.
	68.000
	TON

	GEOTEXTILE UNDER RIPRAP, TYPE V, AOS 0.21-0.43
	237.000
	SY
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	BRIDGE ITEMS:
	
	

	TEST PILE
	2.000
	EA

	CONVENTIONAL STATIC PILE LOAD TEST
	0.000
	EA

	14" PRESTRESSED CONCRETE PILING
	920.000
	LF

	18" PRE-FORMED PILE HOLES
	490.000
	LF

	31 ' PRECAST CONCRETE SLAB UNIT, 3.5 ' INTERIOR
	12.000
	EA

	40 ' PRECAST CONCRETE SLAB UNIT, 3.5 ' INTERIOR
	6.000
	EA

	31 ' PRECAST CONCRETE SLAB UNIT, 3.5 ' EXTERIOR
	4.000
	EA

	40 ' PRECAST CONCRETE SLAB UNIT, 3.5 ' EXTERIOR
	2.000
	EA

	PRECAST CONCRETE BARRIER RAIL
	204.000
	LF

	31.33 ' PRECAST CONCRETE CAP, INTERMEDIATE UNIT, CONCRETE PILE,
	2.000
	EA

	31'' PRECAST CONCRETE CAP, END UNIT, CONCRETE PILE,
	2.000
	EA

	9.25' PRECAST CONCRETE WING
	4.000
	EA

	LOOSE RIPRAP, 300 LB.
	136.000
	TON

	GEOTEXTILE UNDER RIPRAP, TYPE V, AOS 0.21-0.43
	190.000
	SY




	PROJECT NO.
	LSBP-31(22)

	Jasper
	COUNTY



NOTICE TO CONTRACTORS:

	CONTRACT TIME:
	100
	Working Days



The award, if made, will be made to the lowest qualified bidder on the basis of published quantities.

The Board of Supervisors hereby notifies all bidders that it will affirmatively ensure that in any contract entered into pursuant to this advertisement; minority business enterprise will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color, or national origin in consideration for an award.
PLANS AND SPECIFICATIONS are on file in the Office of the Chancery Clerk of Jasper County, LAWRENCE R CLARK , the LSBP Engineer's office and the Office of the State Aid Engineer, 412 E. Woodrow Wilson Avenue, Jackson, Mississippi. This project shall be constructed in accordance with the latest edition of the Mississippi Standard Specifications for State Aid Road and Bridge Construction.
The Plans, Specifications, and Contract documents are on file at the Office of State Aid Road Construction, 412 East Woodrow Wilson Avenue, Jackson, MS 39216 and can be viewed on the OSARC website at www.osarc.gov and obtained online via the website of the County Engineer, Lawrence R. Clark,
P.E. at www.clarkengineersprojects.com. By use of the website the plan holders shall have the option of obtaining hard copy of the Plans and Specifications and/or shall have the opportunity to submit an official bid online. All hard copy proposals shall be directed to the attention of The Jasper County Board of Supervisors with the outside of the envelope marked “Project No. LSBP-31(22) Bid Proposal for Bridge Project”. Contractor shall indicate certificate of responsibility number on the outside of the envelope. Online bids shall be accepted and opened as instructed on the website and in the Contract Documents.



Certified check or bid bond for five percent (5%) of the total bid, made payable to Jasper County and the State of Mississippi must accompany each proposal.


Bidders are hereby notified that any proposal accompanied by letters qualifying in any manner the condition under which the proposal is tendered will be considered an irregular bid and such proposal will not be considered in making the award.



Advertisement Dates: July 22, 2026 & July 29, 2026
	 DOUG ROGERS, President	

	Jasper County Board of Supervisors
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